The parameters and actions are:
 
Integer parameters:
CCR: CCR = 1: Dantzig column choice, 2: Steepest Edge
Current value: 2 Default value: 2. Bounds[1, 2].
ITER_MAX: Maximum number of iterations
Current value: 10000 Default value: 10000. Bounds[1, 1000000000].
RESET_FREQ: Required by EXPAND; shouldn't change
Current value: 10000 Default value: 10000. Bounds[10000, 10000].
K_ITER: Output based on iterations occurs every k_iter iterations
Current value: 1 Default value: 1. Bounds[1, 1000000000].
L_START: Amount of output before iteration starts 0-4
Current value: 0 Default value: 0. Bounds[0, 4].
L_PH1: Amount of output at the end of phase 1 and after reinversion 0-4
Current value: 0 Default value: 0. Bounds[0, 4].
L_END: Amount of output at the end of the run 0-4
Current value: 3 Default value: 3. Bounds[0, 4].
L_ITER: Amount of output every k_iter iterations 0-4
Current value: 0 Default value: 0. Bounds[0, 4].
Float parameters:
REFRESH_FACTOR: refresh_factor * number of rows gives nominal refresh frequency
Current value: 5 Default value: 5. Bounds[1, 10000].
EPSC: tolerance for column choice
Current value: 1e-06 Default value: 1e-06. Bounds[1e-32, 0.0001].
EPSP: tolerance for zero pivot element (t in Gill et al)
Current value: 1e-11 Default value: 1e-11. Bounds[1e-32, 1e-07].
EPSI: tolerance for inversion; should be smaller than EPSP
Current value: 1e-13 Default value: 1e-13. Bounds[1e-32, 1e-08].
EPSB: tolerance for row choices (b values) should = DELF
Current value: 1e-06 Default value: 1e-06. Bounds[1e-06, 1e-06].
EPS: Machine precision ~ DBL_EPSILON = ~2^-52 for IEEE doubles
Current value: 1e-16 Default value: 1e-16. Bounds[1e-32, 0.0001].
DEL0: Initial value for delta (EXPAND)
Current value: 5e-07 Default value: 5e-07. Bounds[5e-07, 5e-07].
TAU: Change in delta each iteration
Current value: 4.9e-13 Default value: 4.9e-13. Bounds[4.9e-13, 4.9e-13].
DELF: Master feasibility tolerance; should be ~ EPS^(3/8) amd = EPSB
Current value: 1e-06 Default value: 1e-06. Bounds[1e-06, 1e-06].
Boolean parameters:
REFRESH_OFF: When 1, on, true, ... turns off reinversion for timing studies
Current value: 0 Default value: 0
RFLAG: Extra debuggin information when non-zero, true, on, ....
Current value: 0 Default value: 0
MAX: If maximizing rather than minimizing
Current value: 0 Default value: 0
Actions:
QUIT: Leaves program
HELP: Used to get help, and values of defaults and bounds.
SHOW: Shows license information: show c->copyright, show w->no warrantee.
